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Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2179 on: September 12, 2014, 02:45:32 PM »

· Quote
http://www.overunity.com/7443/closing-the-loop-on-milkovics-two-stage-mechanical-oscillator/
Start from reply 21…

In analyzing the Milkovic 2 stage pendulum as shown on youtube:
https://www.youtube.com/watch?v=gC6Qlj1Mbo8

We noted that after 2.30 minutes, a single push by the hand will lift the weight twice. On close examination, the lifting of the Weight appeared to be when the pendulum bob is swinging with the maximum velocity at the vertical position. 

In Physics, work is done (energy is spent) only when there is displacement. In this case, the output is the lifting of the weight.


It should now be clear to all experimenters that any overunity measurement or loopback mechanism MUST be done at large angles when the weight is actually lifted.
Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2182 on: September 13, 2014, 12:33:08 AM »

· Quote
Quote from: iacob alex on September 12, 2014, 07:20:20 PM
Hi 888 !
Why not to play the largest possible angle ? ( starting as a free inverted pendulum ).
Al_ex

@Al_ex,
The largest possible angle will be the next stage. In the next stage, the pendulum will be replaced by an unbalanced wheel.

At this stage, it is only necessary to show that the Input Energy by the fingers is less than the Output Energy as shown by the lifting of the Weight (twice). Success at this stage will indicate overunity. Note that the electromagnet can be placed in a fixed position to repel the magnetic pendulum bob when it rises to the exact position. The Weight to be lifted and/or the lever arm can be adjusted so that the system is in balance (or in resonance). This means that the process can be repeated exactly with the pulsing of the electromagnet to provide Input Energy. That Input Energy plus the Lead-out Energy will provide the Output Energy in lifting the Weight and overcome friction and air resistance.
The large setup in the video or similar is a good candidate for the experiment.

I attached the figure showing the large angle to do such an experiment. Has any experimenter used such large angles?


The tension of the pendulum string does the magic twice – leads-out gravitational energy during the push and lifts the Weight with centripetal force when the velocity is highest.
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Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2184 on: September 13, 2014, 06:40:05 AM »

· Quote
Quote from: markdansie on September 13, 2014, 04:48:28 AM
Hi 888
I admire you tenacity and good nature in your pursuit of free energy or overunity. I also find your posts entertaining. However is in not time to do some reflection on your claims, theories and assumptions made over the years that have always never panned out? Perhaps with a review you may see some common areas with miscalculations, misleading assumptions and incorrect conclusions. This may prove to be very valuable by learning from past mistakes in order to assist you in your endeavors in the future. Otherwise we are just faced with the usual garbage in garbage out.
Never stop, I encourage you and everyone else, but sit back and learn from past mistakes.
Kind Regards
Mark Dansie

http://www.alternate-energy.net/Dvid/view.php?video=ArX7BDY1XRM&title=The+225+HP+Pulse+Motor

I posted that video in 2006. That pulse motor was from USA and I explained its operation at Tsinghua University. I also explained the Energy Multiplier from Tsinghua using the Lead-out energy theory. I was investigated as a US spy when I returned to Hong Kong.

Now I have grounds to believe that Pulse Motor was real and used in Army Tanks in China! I shall review my theory and calculations. Since I already have a work bench at Overunityresearch.com, I shall put the updates there. Those who want to see the reviews and check the calulations can visit that site. No comments are allowed at that site but those who want to comment can post here or in a new thread.

The large Milkovic 2 stage pendulum video convinced me that if we treat the finger push as Input and the twice lifting of the Weight as Output, we should have Output > Input. My old mathematical treatment of this pendulum was wrong as it did not consider the moments correctly. I shall revise that.

God Bless.
Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2186 on: September 13, 2014, 02:28:32 PM »

· Quote
Quote from: Paul-R on September 13, 2014, 01:44:18 PM

"the finger push as Input" = force x distance moved

"the twice lifting of the Weight as Output" = m x g x h (twice)

The fact that the weight's potential energy is not saved, but reverts to some noise and heat when it descends makes no difference. I am sure this is right.

The weight's PE needs to be saved and made to do useful work by some means.

@Paul-R,

For the first stage experiment, we just compare the Input Energy with the Output energy. The Output energy dissipated as noise is acceptable. The video makes it very convincing that Input Energy is less than Output Energy. We just need to confirm it with more scientific measurements.

The best point from the video is that overunity can only be demonstrated at large angles with such setup....
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Milkovic 2 stage Pendulum Analysis

W1 = Weight to be lifted
L1 L2 P W2 = Pendulum bob
— T l d P =Pulse Force
. d = displacementof P

T = Tension of String
L =length of Pendulum
L1=Lever Arm 1

L2 = Lever Arm 2
P h : ~ h = Height lifted

W1

INPUT Energy = Pd OUTPUT Energy = Wigh (h = sum of two heights with one pulse)

Tensionis responsible for Lead-out Energy during pulse (Lee-Tseung theory)

and lifting of W1 at maximum Velocity (clockwise moment > anti-clockwise moment)
Can OUTPUT Energy be greater than INPUT Energy?
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Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2190 on: September 14, 2014, 12:00:10 AM »

· Quote
One question raised by a Chinese Experimenter:

Must I build a large 2-stage Milkovic Oscillator to detect or confirm overunity? Can I build a small model in the laboratory?

Answer: When we first pulse the pendulum, the Weight W1 will not rise at all. The Input Energy and Lead-out Energy are all used to increase the amplitude of the Swing. After sufficient build-up, the Weight W1 can be lifted (twice). Output can then be easily measured. The pulsing energy (Pd) is very small. Thus a large 2-stage Milkovic Oscillator is needed to provide a large enough (Pd) for experiment.

Even after the Weight W1 is lifted, there is likely to be some tuning to achieve best results. The adjustment can be via changing the mass of W1 or the Lever Arm L1. Too small a model will not permit such tuning.

This answer is likely to apply to the Pulse Motor later on. The wheel should be large or multiple coupled wheels like the 225 HP motor needs to be used.
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Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2191 on: September 14, 2014, 11:56:55 PM »

· Quote
One comment:
The OUTPUT Energy of the Milkovic 2-stage pendulum is NOT the W1 times g times the total height. The swinging lever is an oscillating system (seesaw). That oscillating system also converts potential energy into kinetic energy and vice versa. 

What should be the correct OUTPUT Energy?
Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2192 on: September 15, 2014, 02:33:22 PM »

· Quote
After examining the video carefully, it is found that the Weight W1 is lifted when the pendulum bob swings at maximum velocity. At this position, the Tension of the String will be the sum of the pendulum bob W2 x g and the extra force due to circular motion (Centrifugal or centripetal force).

The heavier weight W1 (74 pounds) can be lifted by the smaller weight of the pendulum bob (46 pounds). The Lever Arms L1 appear to larger or equal to L2. The anti-clockwise moment due to the Weight W1 time L1 initially is definitely greater. But after build-up, the centrifugal force plus the weight of the pendulum bob will provide a Tension much larger than 74 pounds.

The Lee-Tseung lead-out energy theory considers the pulling up of the Weight W1 as Lead-out gravitational energy. The lever system moves or rotates clockwise resulting in lifting of the Weight W1. Lead-out energy comes at this stage. Some energy transfer takes place as the pivot of the pendulum goes down but this energy is gained back later.

Thus the design of an efficient overunity Milkovic system requires:
1. Pendulum Bob Weight should be less than W1.
2. Pendulum length should be large to get high velocity to provide Centrifugal force.
3. L1 should be greater or equal to L2 to provide an initial larger anti-clockwise moment.
(The video helps to provide such insights.)
Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2194 on: September 15, 2014, 10:55:42 PM »

· Quote
· Modify
Initially, the lever system has no oscillation as the anti-clockwise moment of W1 and L1 is larger.

Then the amplitude of oscillation of the pendulum gets larger, the Tension in the string gets higher because of the higher velocity at the lowest point.
“Suddenly”, the clockwise moment of the pendulum side is larger. The Weight W1 will be lifted. Work is done. Energy goes to the Lever System. Energy of the Lever System can be regarded as (W1 x g x h’) where h’ is the higher of the height raised. 

The Pulsing energy (Pd) can remain the same. It will not impart energy to the lever system until the “critical angle”. At the “critical angle”, the entire lever system energy (W1 x g x h’) appeared.


If we regard the INPUT energy as Pd and the OUTPUT energy as (W1 x g x h’), we can easily get overunity. A 12 time figure is within the possibility.

The observation is that the pendulum system itself is hardly affected with such a “transfer of energy”. Where does such energy come from? One possible explanation is Lead-out Energy. Gravitational energy is brought-in.

We can use the brought-in gravitational energy at the lever system. This will be replenished again by subsequent bringing-in of gravitational energy again!


In conclusion, the varying Tension of the Pendulum String does the magic in two ways:

1. Lead-out some gravitational energy during each pulse.

2. Lead-out more gravitational energy in one big splash after build-up when the clockwise moment is higher.



Divine Revelation?
Re: 12 times more output than input, dual mechanical oscillation system !
« Reply #2196 on: Today at 03:11:38 AM »

· Quote
· Modify
Quote from: zoelra on September 15, 2014, 11:38:14 PM
I can't take this anymore. The lead-out theory is total hogwash. No legitimate/recognized scientific or academic group has ever validated the theory to be true. In all the years of pushing the theory, not one working device has ever been put on display, and no proof of free energy gain from string tension has ever been demonstrated.

In a two stage oscillator, the pendulum swings due to gravity just as the mathematics predicts. Centrifugal force of the swinging pendulum bob is responsible for the raising of the counter weight, and nothing else. Any serious 2SO investigator would know this to be true. Simple potential to kinetic energy conversion and centrifugal force is all that is going on here, all easily confirmed using accepted physics theory and mathematics.

Ok, maybe I was a bit harsh to say the theory is hogwash, but it hasn't been proven, and to claim the 2SO functions because of it is total hogwash. Prove the theory first.

The 225 HP posted in reply 2190 is PROOF already. Both USA and China Military have similar pulse engines. A lot of debunkers were paid to discredit it. 
Scientifically, if the energy of the lever system were provided by the pendulum system, the pendulum system should show a marked decrease in energy. That should be a sudden decrease in the amplitude of oscillation. The video clearly showed that it is NOT the case. Energy must come from somewhere else. Gravitational Energy is Lead-out - one possible explanation.

The book by Jovan Marjanovic is worth reading even though I do not agree with all the points.
Quote:
Basic Principles of Over Unity
Electromagnetic Machines
A Scientific View into the World of Free
Energy from Electric Charges and
Magnetic Fields
by Jovan Marjanovic, M.Sc.
Johann W. Goethe said that the biggest secrets
were the open ones. You look at them but you do
not see them. The same is true with the
electromagnetic field. It is known fact that after
switching off an electromagnet, its magnetic
energy will be returned back to the circuit,
usually as a spark. What was missed is the fact
that the magnetic energy performed work by
attraction of an iron bar and didn’t consume
itself. This work, minus heat losses inside the
circuit, is free energy or over unity energy.

The goal of this book is to unlock the secrets of over unity and to teach people what is over
unity and how it works. The reader will learn basic ideas of making new ultra efficient
electric motors and generators and how to improve existing patents which use permanent
magnets.
More information and ordering
http://books.veljkomilkovic.com

We have all seen the video many times. Only recently, I realized that the lever system energy appeared suddenly - with no apparent change in energy of the pendulum system (no significant amplitude change). Energy must come from elsewhere. Traditional Physics could not explain that. If the total energy is conserved with no outside energy coming in - the pendulum system must lose some energy. The amplitude MUST decrease significantly.
Johann W. Goethe said that the biggest secrets
were the open ones. You look at them but you do
not see them. 

Hopefully, the Divine One opened my eyes this time - after 10 years!
↓
